Update for the Labcycler-Pro to firmware version 00.006.

Instructions:
-------------

Copy the files update.bin and update.bin.sign to the root directory of an USB stick.
Start the Labcycler-Pro and insert the USB stick into the front USB socket.
Then navigate to the settings dialog, select the "Device" tab,
or if no tabs present, scroll a little bit down, and click on the "Update" button.
Afterwards follow the instructions on screen.

Changelog:
-----------

V00.006:
- Fixed error: When using gradients, the temperatures are correct, but are displayed slightly incorrectly (V00.005 claims to also do so, but does not).
- Fixed error: Gradients displayed in step list even if executing on Triple Block.
- Improvement: Added program listing to reports.
- Improvement: Show at least 6 rows in the program table in the monitor and reports.

V00.005:
- Added feature: Differentiation between Gradient and Basic versions.
- Added feature: Support for upgrades from Basic to Gradient versions via license code.
- Improvement. Warn about unused, but  gradients in programs when using a Triple Block.
- Improvement: Show a warning before first editing a program.
- Improvement: Display error message when things unexpectedly go wrong and the device needs to be restarted.
- Improvement: Show a warning when probes are missing.
- Improvement: Deactivate busy blocks in block selection of a Triple Block.
- Improvement: In German, "Protokolle" have been renamed to "Berichte" to avoid misunderstandings.
- Improvement: Consistent use of the formal form in Spanish version.
- Improvement: Support for exfat filesystem added.
- Fixed error: Program- and directorynames containing certain special characters could not be used on flash drives.
- Fixed error: First two digits of the version number are now shown.
- Fixed error: Too few decimal places for cation concentration in the TM dialog.
- Fixed error: Minor typos.
- Fixed error: The manual states that NTFS is supported instead of Fat32 as the file system.
- Fixed error: When using gradients, the center temperature is correct, but is displayed slightly incorrectly.

V00.004:
- Added feature: Graphic programming
- Improvement: Redesign of settings with content grouped with tabs.
- Improvement: Changed background color of info overlay containing valid ranges for input fields from red to blue.
- Improvement: New programs are made of a single step.
- Improvement: Language-dependent position of keys 'x' and 'y' for alpha keyboard.
- Improvement: Expansion of help texts.
- Improvement: Key to switch to numeric keypad is now labeled "!#1".
- Improvement: input fields are highlighted for a longer period of time when using undo and redo functionality. 
- Fixed error: Crashing on starting a program with no pressure specified.
- Fixed error: Remove all reports does not ask and needs restart to take effect.
- Fixed error: Gradient only +-10 °C instead of +-20°C.
- Fixed error: No values shown in Info tab of a report with german language selected.
- Fixed error: Graphic in reports does only show first channel instead of all three.
- Fixed error: Local folder not showing special Icon.
- Fixed error: Text of copy button not visible when disabled and already copying.
- Fixed Error: Label "48" instead of "48Al" for silver block.
- Fixed error: Entry for V00.003 in changelog is missing.

V00.003:
- Fixed error: Some blocks are not sufficiently supported (introduced in V00.002).

V00.002 (Not released):
- Added feature: Block monitor icon on side tab is orange if a block is running.
- Fixed error: Incorrect step counter when using a Triple Block.
- Fixed error: All graphs are removed when a new program is started on a Triple Block.
- Fixed error: Points are added to graphs of channel which is not currently running using a Triple Block. 
- Fixed error: Graph of finished program executions are visible.
- Fixed error: Max graph length of 1 hours and 30 min instead of 4 hours.
- Fixed error: Graphs a little bit scrollable with no or small program run.
- Fixed error: Wrong colors on single graph with Triple Block.
- Fixed error: Middle graph thicker on Triple Block graph.
